A Big Earth Data Platform for Three Poles

**Cold and Arid Research Network of Lanzhou university (eddy covariance system of Minqin station, 2019)**

1、Description

This dataset contains the flux measurements from the Minqin station eddy covariance system (EC) in the middle reaches of the Shiyanghe integrated observatory network from August 29 to December 31 in 2019. The site (103.668E, 39.208N) was located on a alpine meadow in the Wuwei, Gansu Province. The elevation is 1020 m. The EC was installed at a height of 4.0 m, and the sampling rate was 10 Hz. The sonic anemometer faced north, and the separation distance between the sonic anemometer and the CO2/H2O gas analyzer (CSAT3&Li7500A) was 0.17 m.
The raw data acquired at 10 Hz were processed using the Eddypro post-processing software, including the spike detection, lag correction of H2O/CO2 relative to the vertical wind component, sonic virtual temperature correction, coordinate rotation (2-D rotation), corrections for density fluctuation (Webb-Pearman-Leuning correction), and frequency response correction. The EC data were subsequently averaged over 30 min periods. The observation data quality was divided into three classes according to the quality assessment method of stationarity (Δst) and the integral turbulent characteristics test (ITC): class 1-3 (high quality), class 4-6 (good), class 7-8 (poor, better than gap filling data), class9 (rejected). In addition to the above processing steps, the half-hourly flux data were screened in a four-step procedure: (1) data from periods of sensor malfunction were rejected; (2) incomplete 30 min data were rejected when the missing data constituted more than 3% of the 30 min raw record; and data were rejected at night when the friction velocity (u\*) was less than 0.1 m/s. There were 48 records per day, and the missing data were replaced with -6999. Suspicious data were marked in red.
The released data contained the following variables: data/time, wind direction (Wdir, °), wind speed (Wnd, m/s), the standard deviation of the lateral wind (Std\_Uy, m/s), virtual temperature (Tv, ℃), H2O mass density (H2O, g/m3), CO2 mass density (CO2, mg/m3), friction velocity (ustar, m/s), stability (z/L), sensible heat flux (Hs, W/m2), latent heat flux (LE, W/m2), carbon dioxide flux (Fc, mg/ (m2s)), quality assessment of the sensible heat flux (QA\_Hs), quality assessment of the latent heat flux (QA\_LE), and quality assessment of the carbon flux (QA\_Fc). In this dataset, the time of 0:30 corresponds to the average data for the period between 0:00 and 0:30; the data were stored in \*.xls format. Detailed information can be found in the suggested references.

2、Keywords

Theme：Latent heat flux,Radiation,Carbon dioxide flux,Sensible heat flux
Discipline：Atmosphere
Places：Shiyang River Basin
Time：2019

3、Data details

1.Scale：None

2.Projection：

3.Filesize：1.08MB

4.Data format：None

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：39.208 | - |
| west：103.668 | - | east：103.668 |
| - | south：39.208 | - |

5、Time frame:2020-03-14 00:00:00+00:00--2020-07-16 00:00:00+00:00

6、Reference method

References to data:

ZHANG Renyi, ZHAO Changming. Cold and Arid Research Network of Lanzhou university (eddy covariance system of Minqin station, 2019). A Big Earth Data Platform for Three Poles, doi:10.11888/Meteoro.tpdc.2707892020

References to articles:

7、Supporting project information

Pan-Third Pole Environment Study for a Green Silk Road-A CAS Strategic Priority A Program

8、Data resource provider

name: ZHAO Changming
unit: Lanzhou University
email: zhaochm@lzu.edu.cn

name: ZHANG Renyi
unit: Lanzhou University
email: zrenyi@lzu.edu.cn