A Big Earth Data Platform for Three Poles

**Qilian Mountains integrated observatory network: Cold and Arid Research Network of Lanzhou university (an observation system of meteorological elements gradient of Sidalong Station, 2018)**

1、Description

This dataset includes data recorded by the Cold and Arid Research Network of Lanzhou university obtained from an observation system of Meteorological elements gradient of Sidalong Station from October 24 to December 31, 2018. The site (38.430°E, 99.931°N) was located on a forest in the Kangle Sunan, which is near Zhangye city, Gansu Province. The elevation is 3059 m. The installation heights and orientations of different sensors and measured quantities were as follows: air temperature and humidity profile (0.5, 3, 13, 24, and 48 m), wind speed and direction profile (windsonic; 0.5, 3, 13, 24, and 48 m), air pressure (1.5 m), rain gauge (24 m), infrared temperature sensors (4 m and 24m, vertically downward), photosynthetically active radiation (4 m and 24m), soil heat flux (-0.05 m and -0.1m), soil temperature/ moisture/ electrical conductivity profile -0.05, -0.1m, -0.2m, -0.4m and -0.6mr), four-component radiometer (24 m, towards south), sunshine duration sensor(24 m, towards south).
The observations included the following: air temperature and humidity (Ta\_0.5 m, Ta\_3 m, Ta\_13 m, Ta\_24 m, and Ta\_48 m; RH\_0.5 m, RH\_3 m, RH\_13 m, RH\_24 m, and RH\_48 m) (℃ and %, respectively), wind speed (Ws\_0.5 m, Ws\_3 m, Ws\_13 m, Ws\_24 m, and Ws\_48 m) (m/s), wind direction (WD\_0.5 m, WD\_3 m, WD\_13 m, WD\_24 m, and WD\_48 m) (°), air pressure (press) (hpa), precipitation (rain) (mm), four-component radiation (DR, incoming shortwave radiation; UR, outgoing shortwave radiation; DLR\_Cor, incoming longwave radiation; ULR\_Cor, outgoing longwave radiation; Rn, net radiation) (W/m^2), infrared temperature (IRT\_A, IRT\_B) (℃), photosynthetically active radiation (PAR\_A, PAR\_B) (μmol/ (s m^2)), soil heat flux (Gs\_0.05m, Gs\_0.1m) (W/m^2), soil temperature (Ts\_5 cm, Ts\_10 cm, Ts\_20 cm, Ts\_40 cm, and Ts\_60 cm) (℃), soil moisture (Ms\_5 cm, Ms\_10 cm, Ms\_20 cm, Ms\_40 cm, and Ms\_60 cm) (%, volumetric water content),soil water potential (SWP\_5cm, SWP\_10cm, SWP\_20cm, SWP\_40cm, and SWP\_60cm)(kpa), soil conductivity (Ec\_5cm, Ec\_10cm, Ec\_20cm, Ec\_40cm, and Ec\_60cm)(μs/cm), sun time (h).
The data processing and quality control steps were as follows: (1) The AWS data were averaged over intervals of 10 min for a total of 144 records per day. The soil water potential in the area is so low that it has exceeded the sensor measurements. (2) Data in duplicate records were rejected. (3) Unphysical data were rejected. (4) The data marked in red are problematic data. (5) The format of the date and time was unified, and the date and time were collected in the same column, for example, date and time: 2018-6-10 10:30.

2、Keywords

Theme：Precipitation,Desert,Vegetation,Meteorological element
Discipline：Atmosphere,Terrestrial Surface
Places：Heihe River Basin
Time：2018

3、Data details

1.Scale：None

2.Projection：None

3.Filesize：3.85MB

4.Data format：None

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：38.428 | - |
| west：99.926 | - | east：99.926 |
| - | south：38.428 | - |

5、Time frame:2018-01-12 16:00:00+00:00--2019-01-11 16:00:00+00:00

6、Reference method

References to data:

ZHANG Renyi, ZHAO Changming. Qilian Mountains integrated observatory network: Cold and Arid Research Network of Lanzhou university (an observation system of meteorological elements gradient of Sidalong Station, 2018). A Big Earth Data Platform for Three Poles, doi:10.11888/Geogra.tpdc.2701472019

References to articles:

7、Supporting project information

Pan-Third Pole Environment Study for a Green Silk Road-A CAS Strategic Priority A Program

8、Data resource provider

name: ZHAO Changming
unit: Lanzhou University
email: zhaochm@lzu.edu.cn

name: ZHANG Renyi
unit: Lanzhou University
email: zrenyi@lzu.edu.cn