A Big Earth Data Platform for Three Poles

**HiWATER: Dataset of hydrometeorological observation network (No.4 runoff observation system of Wujing bridge on the Heihe River, 2013)**

1、Description

The No. 4 hydrological section is located at Wujin Heihe River Bridge (100.433° E, 39.065° N, 1431 m) in the midstream of the Heihe River Basin, Zhangye city, Gansu Province. The dataset contains recorded by the No.4 hydrological section from 10 June, 2012 to 10 August, 2012, and from 6 September, 2013 to 31 December, 2013. The width of this section is 58 meters and the cross-sectional area is unstable because of human factors. The water level was measured using an HOBO pressure range and the discharge was measured using cross-section reconnaissance by the StreamPro ADCP. The dataset includes the following parameters: water level (recorded every 30 minutes) and discharge. The missing and incorrect (outside the normal range) data were replaced with -6999.
For more information, please refer to Li et al. (2013) (for hydrometeorological observation network or sites information), He et al. (2016) (for data processing) in the Citation section.

2、Keywords

Theme：Surface Water,Hydrology section,Discharge/Flow,Runoff
Discipline：Terrestrial Surface
Places：Heihe River Basin, the artificial oasis experimental area in the middle reaches,
Time：2013-09-06 to 2013-12-31, 2013, 2012-06-14 to 2012-11-24

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：0.55MB

4.Data format：EXCEL

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：39.065 | - |
| west：100.4325 | - | east：100.433056 |
| - | south：39.064722 | - |

5、Time frame:2012-06-20 16:00:00+00:00--2012-11-30 16:00:00+00:00

6、Reference method

References to data:

LI Xin, LIU Shaomin, XU Ziwei, HE Xiaobo. HiWATER: Dataset of hydrometeorological observation network (No.4 runoff observation system of Wujing bridge on the Heihe River, 2013). A Big Earth Data Platform for Three Poles, doi:10.3972/hiwater.213.2014.db2016

References to articles:

Li, X., Cheng, G.D., Liu, S.M., Xiao, Q., Ma, M.G., Jin, R., Che, T., Liu, Q.H., Wang, W.Z., Qi, Y., Wen, J.G., Li, H.Y., Zhu, G.F., Guo, J.W., Ran, Y.H., Wang, S.G., Zhu, Z.L., Zhou, J., Hu, X.L., & Xu, Z.W. (2013). Heihe watershed allied telemetry experimental research (hiwater): scientific objectives and experimental design. Bulletin of the American Meteorological Society, 94(8), 1145-1160. doi:10.1175/BAMS-D-12-00154.1.

Liu, S.M., Li, X., Xu, Z.W., Che, T., Xiao, Q., Ma, M.G., Liu, Q.H., Jin, R., Guo, J.W., Wang, L.X., Wang, W.Z., Qi, Y., Li, H.Y., Xu, T.R., Ran, Y.H., Hu, X.L., Shi, S.J., Zhu, Z.L., Tan, J.L., Zhang, Y., & Ren, Z.G. (2018). The Heihe Integrated Observatory Network: A Basin-Scale Land Surface Processes Observatory in China. Vadose Zone Journal, 17(1), 180072. doi:10.2136/vzj2018.04.0072.

7、Supporting project information

National Natural Science Foundation of China

8、Data resource provider

name: XU Ziwei
unit: Beijing Normal University
email: xuzw@bnu.edu.cn

name: HE Xiaobo
unit: Cold and Arid Regions Environmental and Engineering Research Institute, Chinese Academy of Sciences
email: hxb@lzb.ac.cn

name: LI Xin
unit:
email: xinli@itpcas.ac.cn

name: LIU Shaomin
unit: Beijing Normal University
email: smliu@bnu.edu.cn