A Big Earth Data Platform for Three Poles

**WATER: Dataset of airborne LiDAR mission at the super site in the Dayekou watershed flight zone on Jun. 23, 2008**

1、Description

The dataset of airborne LiDAR mission at the super site in the Dayekou watershed flight zone on Jun. 23, 2008 included peak pulse data (\*.LAS), full waveform data (.lgc), CCD photos, DEM, DSM and DOM. The flight routes were as follows:  
  
{|  
! flight route   
! startpoint lat  
! startpoint lon  
! endpoint lat  
! endpoint lon  
! altitude (m)  
! length (km)  
! photos  
|-  
| 1 || 38°31′59.71″ || 100°14′54.02″ || 38°31′43.04″ || 100°15′44.28″ || 3550 || 1.3 || 7  
|-  
| 2 || 38°32′01.21″ || 100°14′54.82″ || 38°31′44.53″ || 100°15′45.08″ || 3550 || 1.3 || 7  
|-  
| 3 || 38°32′02.70″ || 100°14′55.62″ || 38°31′46.03″ || 100°15′45.88″ || 3550 || 1.3 || 7  
|-  
| 4 || 38°32′04.20″ || 100°14′56.42″ || 38°31′47.52″ || 100°15′46.69″ || 3550 || 1.3 || 7  
|-  
| 5 || 38°32′05.69″ || 100°14′57.23″ || 38°31′49.01″ || 100°15′47.49″ || 3550 || 1.3 || 6  
|}

2、Keywords

Theme：Airborne laser radar,Remote Sensing Technology,CCD  
Discipline：Remote Sensing Technology  
Places：Heihe River Basin, Dayekou watershed foci experimental areas, Forest and Hydrology Experimental Areas  
Time：2008,

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：14999.8MB

4.Data format：

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：38.75 | - |
| west：100.15 | - | east：100.5 |
| - | south：38.45 | - |

5、Time frame:2018-11-24 02:50:15+00:00--2018-11-24 02:50:15+00:00

6、Reference method

References to data:

LI Xin, MA Mingguo, LIU Qingwang, FAN Fengyun, BAO Yunfei, Liu Qiang, ZHOU Mengwei, NI Wenjian, HE Qisheng, LI Shiming, CHI Hong, PANG Yong, WANG Tao. WATER: Dataset of airborne LiDAR mission at the super site in the Dayekou watershed flight zone on Jun. 23, 2008. A Big Earth Data Platform for Three Poles, doi:10.3972/water973.0220.db2013

References to articles:

何祺胜, 陈尔学, 曹春香, 刘清旺, 庞勇. 基于LIDAR数据的森林参数反演方法研究. 地球科学进展, 2009, 24(7): 748-755.  
  
刘清旺. 机载激光雷达森林参数估测方法研究. 北京: 中国林业科学研究院, 2009.  
  
Tian, X., Li, Z.Y., van der Tol C, Su, Z., Li, X., He, Q.S., Bao, Y.F., Chen, E.X., & Li, L.H. (2011). Estimating zero-plane displacement height and aerodynamic roughness length using synthesis of LiDAR and SPOT-5 data. Remote Sensing of Environment, 115(9): 2330-2341. 10.1016/j.rse.2011.04.033.  
  
Liu QW, Li ZY, Chen EX, Pang Y, Li SM, Tian X. Feature analysis of LIDAR waveforms from forest canopies. Science China-earth Sciences, 2011, 54(8): 1206-1214. 10.1007/s11430-011-4212-3.  
  
刘清旺, 李增元, 陈尔学, 庞勇, 李世明, 田昕. 森林冠层探测激光雷达的波形特征分析. 中国科学：地球科学, 2011, 41(11): 1670-1678.

7、Supporting project information

The CAS (Chinese Academy of Sciences) Action Plan for West Development Project  
National Program on Key Basic Research Project (973 Program

8、Data resource provider

name: MA Mingguo  
unit: Cold and Arid Regions Environmental and Engineering Research Institute, Chinese Academy of Sciences  
email: mmg@lzb.ac.cn  
  
name: LI Xin  
unit:   
email: xinli@itpcas.ac.cn  
  
name: BAO Yunfei  
unit: Beijing Normal University  
email:   
  
name: NI Wenjian  
unit: Beijing Normal University  
email:   
  
name: Liu Qiang  
unit:   
email:   
  
name: LIU Qingwang  
unit: Chinese Academy of Forestry  
email: liuqw@caf.ac.cn  
  
name: HE Qisheng  
unit:   
email: hqsfei999@163.com  
  
name: WANG Tao  
unit:   
email:   
  
name: CHI Hong  
unit:   
email:   
  
name: ZHOU Mengwei  
unit:   
email: mengweizhou@hotmail.com  
  
name: FAN Fengyun  
unit:   
email:   
  
name: PANG Yong  
unit:   
email:   
  
name: LI Shiming  
unit:   
email: