A Big Earth Data Platform for Three Poles

**HiWATER: Dataset of hydrometeorological observation network (eddy covariance system of Populus forest station, 2014)**

1、Description

This dataset contains eddy correlation instrument observation data from the Huyanglin station downstream of the Heihe Hydrological and Meteorological Observation Network from January 1, 2014 to December 31, 2014. The site is located in Sidaoqiao, Ejin Banner, Inner Mongolia, and the underlying surface is Populus euphratica. The latitude and longitude of the observation point is 101.1236E, 41.9928N, and the altitude is 876m. The vortex correlator has a height of 22 m and a sampling frequency of 10 Hz. The ultrasonic orientation is in the north direction, and the distance between the ultrasonic wind speed temperature meter (CSAT3) and the CO2/H2O analyzer (Li7500) is 17 cm.
The original observation data of the eddy correlation meter is 10 Hz, and the released data is 30 minutes of data processed by Eddypro software. The main steps of the processing include: outlier removal, time-lag correction, coordinate rotation (secondary coordinate rotation), frequency response correction, ultrasonic virtual temperature correction and density (WPL) correction, etc. At the same time, the quality evaluation of each flux value is conducted, it mainly contains atmosphere state stability test(Δst) and integrated turbulence characteristic test(ITC).
The 30-min flux value output by Eddypro software was also screened: (1) data from the instrument error was eliminated; (2) data 1 h before and after precipitation was removed; (3) data from the deletion rate greater than 10% within every 30 min of the 10 Hz raw data. (4) eliminating observation data of weak turbulence at night (u\* less than 0.1 m/s). The average time period of observation data is 30 minutes, 48 data per day, and the missing data is labeled -6999. Abnormal data caused by instrument drift and other reasons are marked in red. From February 21 to March 13, the data is missing due to problems in memory card and wireless transmission module.
Published observations include: date/time Date/Time, wind direction Wdir(°), horizontal wind speed Wnd(m/s), lateral wind speed standard deviation Std\_Uy(m/s), ultrasonic virtual temperature Tv(°C), water vapor density H2O (g/m3), carbon dioxide concentration CO2 (mg/m3), friction velocity Ustar (m/s), stability Z/L (dimensionless), sensible heat flux Hs (W/m2), latent heat flux LE (W/m2), carbon dioxide flux Fc (mg/(m2s)), sensible heat flux quality identification QA\_Hs, latent heat flux quality identification QA\_LE, carbon dioxide flux quality identification QA\_Fc. The quality identification of sensible heat, latent heat, and carbon dioxide flux is divided into three levels (quality mark 0: (Δst <30, ITC<30); 1: (Δst <100, ITC<100); the rest is 2). The meaning of the data time, such as 0:30 represents an average of 0:00-0:30; the data is stored in \*.xls format.
For hydrometeorological network or site information, please refer to Li et al. (2013). For observation data processing, please refer to Liu et al. (2011).

2、Keywords

Theme：Latent heat flux,Radiation,Carbon dioxide flux,Sensible heat flux
Discipline：Atmosphere
Places：Heihe River Basin, populus forest station, the natural oasis eco-hydrology experimental area in the lower reaches
Time：2014, 2014-01-01 to 2014-12-31

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：1.2MB

4.Data format：文本

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：41.9928 | - |
| west：101.1236 | - | east：101.1236 |
| - | south：41.9928 | - |

5、Time frame:2014-01-10 00:00:00+00:00--2015-01-09 00:00:00+00:00

6、Reference method

References to data:

TAN Junlei, LI Xin, LIU Shaomin, XU Ziwei, CHE Tao, REN Zhiguo. HiWATER: Dataset of hydrometeorological observation network (eddy covariance system of Populus forest station, 2014). A Big Earth Data Platform for Three Poles, doi:10.3972/hiwater.239.2015.db2016

References to articles:

Liu, S.M., Xu, Z.W., Wang, W.Z., Bai, J., Jia, Z., Zhu, M., & Wang, J.M. (2011). A comparison of eddy-covariance and large aperture scintillometer measurements with respect to the energy balance closure problem. Hydrology and Earth System Sciences, 15(4), 1291-1306.

Liu, S.M., Li, X., Xu, Z.W., Che, T., Xiao, Q., Ma, M.G., Liu, Q.H., Jin, R., Guo, J.W., Wang, L.X., Wang, W.Z., Qi, Y., Li, H.Y., Xu, T.R., Ran, Y.H., Hu, X.L., Shi, S.J., Zhu, Z.L., Tan, J.L., Zhang, Y., & Ren, Z.G. (2018). The Heihe Integrated Observatory Network: A Basin-Scale Land Surface Processes Observatory in China. Vadose Zone Journal, 17(1), 180072. doi:10.2136/vzj2018.04.0072.

7、Supporting project information

National Natural Science Foundation of China

8、Data resource provider

name: XU Ziwei
unit: Beijing Normal University
email: xuzw@bnu.edu.cn

name: TAN Junlei
unit:
email: tanjunlei@163.com

name: REN Zhiguo
unit: Cold and Arid Regions Environmental and Engineering Research Institute, Chinese Academy of Sciences
email:

name: LI Xin
unit:
email: xinli@itpcas.ac.cn

name: LIU Shaomin
unit: Beijing Normal University
email: smliu@bnu.edu.cn

name: CHE Tao
unit:
email: chetao@lzb.ac.cn