A Big Earth Data Platform for Three Poles

**Multi-frequency and multi-angular ground-based microwave radiometer and surface parameters experimental data for cropland in 2017**

1、Description

This data set was collected in summer 2017 during the ground-based microwave radiometry experiment, which is part of the Soil Moisture Experiment in the Luan River (SMELR). The experiment site is located in Duolun County, Inner Mongolia (116.47°E, 42.18°N, at 1269 m in altitude). The data set contains three parts, namely brightness temperature data, soil data and vegetation data. The microwave brightness temperature data was observed by a vehicle-mounted dual-polarized multi-frequency radiometer (RPG-6CH-DP), including the horizontal (H) and vertical (V) polarization brightness temperatures at L-, C- and X-bands. The brightness temperature data were acquired from 30° to 65° with an interval of 2.5°, and the time resolution is 0.5 hours. Soil data contains 5 layers of soil moisture and soil temperature (2.5 cm, 10 cm, 20 cm, 30 cm, 50 cm) over three croplands (corn, oats, and buckwheat), with sampling intervals of 10 minutes. The soil data also contains soil surface roughness, rainfall, irrigation flags, and soil texture. Vegetation data contains leaf area index, plant height, vegetation water content, etc.
The experimental period lasted from July 19 to August 30, 2017, and it provided important data for the land surface microwave radiation modeling and validation, as well as the development of soil moisture retrieval algorithms.

2、Keywords

Theme：Soil,Surface Water,Remote Sensing Technology,Soil moisture,Soil moisture/Water content,Ground-based microwave radiometer
Discipline：Terrestrial Surface,Remote Sensing Technology
Places：Duolun County, Shandian River Watershed
Time：2017year

3、Data details

1.Scale：None

2.Projection：

3.Filesize：3.05MB

4.Data format：None

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：42.18 | - |
| west：116.47 | - | east：116.47 |
| - | south：42.18 | - |

5、Time frame:2017-07-18 16:00:00+00:00--2017-08-30 03:59:59+00:00

6、Reference method

References to data:

GENG Deyuan, HU Lu, SHI Jiancheng, WANG Pingkai, ZHAO Tianjie, FAN Dong, LI Shangnan. Multi-frequency and multi-angular ground-based microwave radiometer and surface parameters experimental data for cropland in 2017. A Big Earth Data Platform for Three Poles, doi:10.11888/Soil.tpdc.2716222021

References to articles:

Zhao, T.J., Shi, J.C., Lv, L.Q., Xu, H.X., Chen, D.Q., Cui, Q., Jackson, T.J., Yan, G.J., Jia, L., Chen, L.F., Zhao, K., Zheng, X.M., Zhao, L.M., Zheng, C.L., Ji, D.B., Xiong, C., Wang, T.X., Li, R., Pan, J.M., Wen, J.G., Yu, C., Zheng, Y.M., Jiang, L.M., Chai, L.N., Lu, H., Yao, P.P., Ma, J.W., Lv, H.S., Wu, J.J., Zhao, W., Yang, N., Guo, P., Li, Y.X., Hu, L., Geng, D.Y., & Zhang, Z.Q. (2020). Soil moisture experiment in the Luan River supporting new satellite mission opportunities. Remote Sensing of Environment, 240, 111680

Zhao, T.J., Shi, J.C., Entekhabi, D., Jackson, T.J., Hu, L., Peng, Z.Q., Yao, P.P., Li, S.N., & Kang, C.S. (2021). Retrievals of soil moisture and vegetation optical depth using a multi-channel collaborative algorithm. Remote Sensing of Environment, 257, 112321.

胡路, 赵天杰, 施建成, 李尚楠, 樊东, 王平凯, 耿德源, 肖青, 崔倩, 陈德清. (2020). 基于地基微波辐射观测的土壤水分反演算法评估. 遥感技术与应用, 35(01), 74-84.

Zhao, T.J., Hu, L., Shi, J.C., Lü, H.S., Li, S.N., Fan, D., Wang, P.K., Geng, D.Y., Kang, C.S., & Zhang, Z.Q. (2020). Soil moisture retrievals using L-band radiometry from variable angular ground-based and airborne observations. Remote Sensing of Environment, 248, 111958.

赵天杰, 施建成, 徐红新, 孙彦龙, 陈德清, 崔倩, 贾立, 黄硕, 牛升达, 李秀伟, 阎广建, 陈良富, 柳钦火, 赵凯, 郑兴明, 赵利民, 郑超磊, 姬大彬, 熊川, 王天星, 李睿, 潘金梅, 闻建光, 穆西晗, 余超, 郑姚闽, 蒋玲梅, 柴琳娜, 卢麾, 姚盼盼, 马建威, 吕海深, 武建军, 赵伟, 杨娜, 郭鹏, 李玉霞, 胡路, 耿德源, 张子谦,胡建峰, 杜爱萍. (2021). 闪电河流域水循环和能量平衡遥感综合试验. 遥感学报, 25(4), 871-887.

阎广建, 赵天杰, 穆西晗, 闻建光, 庞勇, 贾立, 张永光, 陈德清, 姚崇斌, 曹志宇, 雷永荟, 姬大彬, 陈良富,柳钦火, 吕利清, 陈镜明, 施建成. (2021). 滦河流域碳、水循环和能量平衡遥感综合试验总体设计. 遥感学报, 25(4), 856-870.

李尚楠, 赵天杰, 施建成, 肖青, 胡路, 王平凯, 赵瑞, 陈德清, 崔倩, 薛淑琴, 胡建峰. (2018). 基于车载微波辐射计的地面观测试验方法. 上海航天, 35(02), 81-90.

7、Supporting project information

Satellite observation and simulation studies of the land surface water and energy exchange processes and its effects on global changes
Application of Remote Sensing in Water Resources Management in Northeast Thailand

8、Data resource provider

name: SHI Jiancheng
unit:
email: shijiancheng@nssc.ac.cn

name: ZHAO Tianjie
unit:
email: zhaotj@aircas.ac.cn

name: HU Lu
unit:
email: hulu@smail.nju.edu.cn

name: LI Shangnan
unit:
email: lisn15@mails.jlu.edu.cn

name: FAN Dong
unit:
email: fandong18@.ucas.ac.cn

name: WANG Pingkai
unit:
email: wangpkjob@gmail.com

name: GENG Deyuan
unit:
email: gengdeyuan@thupdi.com